

**Press to Exit Button**

**Features**:

* Brushed Stainless Steel
* Raised green button
* Legend: Press-to-Exit
* Flush mount
* COM-N/O / COM-N/C

**Dimensions**

 

**Specifications**

* Max. rating 5A/125/250 Vac.
* Contact resistance: 50mΩ Max. (Initial).
* Operating travel: 2.7mm
* Operating life (Mechanical): Over 100,000 times.
* Cables included.