****

**TRUNKING EXTENDED FIRE CLIP 22mm**

**Features**

* 18th Edition Compliant
* Exova Warringtonfire
* Fire Rated for 2 Hours at 970°C
* Certified to BS8434-2
* BS5839-1 Compliant
* Available for use with standard trunking sizes
* Maintains adequate support at high temperatures
* Prevents cable collapse in fire situations
* Test reports available on request.
* Can be fitted retrospectively

**Additional Information**

|  |  |
| --- | --- |
| Trunking Size | 25mm x 16mm |
|  | 38mm x 25mm |
|  | 50mm x 50mm |
|  |  |

