**Smart Bar UIA1000**




## Key Features

* Support Ultra 265/H.265/H.264 video formats
* Face blacklist and whitelist function, can import 5 face blacklist/whitelist libraries.
* 4-channel real-time face comparison
* Real-time blacklist/whitelist face recognition alarm
* Monitoring management
* Tested in different scenes and proved scene-adaptiveness
* Small and light, low power, power saving

## Specifications

|  |  |
| --- | --- |
| **Item** | **UIA1000** |
| Video format | H.265, H.264 |
| Function | Face recognition, real-time monitoring |
| Capacity | Up to 5 blacklist/whitelist libraries with up to 10000 face photos |
| USB interface | USB 3.0 |
| Power supply | USB power supply  Power consumption ≤ 1.5 W |
| Working environment | Temperature: -10°C ~ + 55°C ( +14°F ~ +131°F )  Humidity: ≤ 90% RH (non-condensing) |
| Dimensions(W×D×H) | 89.3mm ×21.0mm ×9.8mm (3.52"×0.83"×0.39") |
| Weight | < 30g ( 0.07 lb ) |

## Dimensions



Zhejiang Uniview Technologies Co.,Ltd.

Building No.10, Wanlun Science Park, Jiangling Road 88, Binjiang District, Hangzhou, Zhejiang, China

Email: [overseasbusiness@uniview.com](mailto:overseasbusiness@uniview.com);globalsupport@uniview.com

http://www.uniview.com

©2018 Zhejiang Uniview Technologies Co.,Ltd. All rights reserved.

\*Product specifications and availability are subject to change without notice.